From 5b52abaa8529f7493f9d4ecf402e9ee130f4f8d2 Mon Sep 17 00:00:00 2001
From: Ron Nazarov <ron@noisytoot.org>
Date: Sat, 14 Feb 2026 20:13:01 +0000
Subject: [PATCH 45/48] mb/supermicro/x11-lga1151-series: Disable ME HECI in
 devicetree

Since we always use me_cleaner, this speeds up boot time by preventing
coreboot from wasting a few seconds waiting for HECI.

Change-Id: Ifbb16ba9f09129795dabe7861260ea4d995c0350
Signed-off-by: Ron Nazarov <ron@noisytoot.org>
---
 src/mainboard/supermicro/x11-lga1151-series/devicetree.cb | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/src/mainboard/supermicro/x11-lga1151-series/devicetree.cb b/src/mainboard/supermicro/x11-lga1151-series/devicetree.cb
index fbf896c6ae..aa09a41f2f 100644
--- a/src/mainboard/supermicro/x11-lga1151-series/devicetree.cb
+++ b/src/mainboard/supermicro/x11-lga1151-series/devicetree.cb
@@ -15,7 +15,7 @@ chip soc/intel/skylake
 		device ref sa_thermal on end
 		device ref south_xhci on end
 		device ref thermal on end
-		device ref heci1 on end
+		device ref heci1 off end
 		device ref sata on
 			register "SataSalpSupport" = "1"
 			register "SataPortsEnable" = "{
-- 
2.47.3

