From 57630265c7ba2429a8215757330348733c087db3 Mon Sep 17 00:00:00 2001
From: Leah Rowe <leah@libreboot.org>
Date: Mon, 21 Apr 2025 05:14:45 +0100
Subject: [PATCH 34/40] Conditional TBFW setting for T480/T480S

Otherwise, other boards will define it, which
might trigger the vendor download script, and
lead to a non-zero exit.

Signed-off-by: Leah Rowe <leah@libreboot.org>
---
 src/mainboard/lenovo/Kconfig | 4 ++++
 1 file changed, 4 insertions(+)

diff --git a/src/mainboard/lenovo/Kconfig b/src/mainboard/lenovo/Kconfig
index 512b326381..3d3490b35d 100644
--- a/src/mainboard/lenovo/Kconfig
+++ b/src/mainboard/lenovo/Kconfig
@@ -18,6 +18,8 @@ config MAINBOARD_FAMILY
 	string
 	default MAINBOARD_PART_NUMBER
 
+if BOARD_LENOVO_T480 || BOARD_LENOVO_T480S
+
 config LENOVO_TBFW_BIN
 	string "Lenovo ThunderBolt firmware bin file"
 	default ""
@@ -44,4 +46,6 @@ config LENOVO_TBFW_BIN
 	  Just leave this blank if you don't care about this option. It's not
 	  useful for every ThinkPad, only certain models.
 
+endif # BOARD LENOVO_T480 || BOARD_LENOVO_T480S
+
 endif # VENDOR_LENOVO
-- 
2.47.3

