From 20921eb7165b23e7b78e4c4126ff5bab8725404b Mon Sep 17 00:00:00 2001
From: Angel Pons <th3fanbus@gmail.com>
Date: Mon, 10 May 2021 22:40:59 +0200
Subject: [PATCH 16/40] nb/intel/gm45: Make DDR2 raminit work

List of changes:
 - Update some timing and ODT values
 - Patch RCOMP calibration to better match what MRC binaries do
 - Replay a hardcoded list of RCOMP codes after RcvEn

This makes raminit work at DDR2-800 speeds and fixes S3 resume as well.
Tested on Toshiba Satellite A300-1ME with two 2 GiB DDR2-800 SO-DIMMs.

Change-Id: Ibaee524b8ff652ddadd66cb0eb680401b988ff7c
Signed-off-by: Angel Pons <th3fanbus@gmail.com>
---
 src/northbridge/intel/gm45/gm45.h             |  2 +-
 src/northbridge/intel/gm45/raminit.c          | 90 +++++++++++++++++--
 .../intel/gm45/raminit_rcomp_calibration.c    | 27 ++++--
 3 files changed, 106 insertions(+), 13 deletions(-)

diff --git a/src/northbridge/intel/gm45/gm45.h b/src/northbridge/intel/gm45/gm45.h
index 5d9ac56606..338260ea7a 100644
--- a/src/northbridge/intel/gm45/gm45.h
+++ b/src/northbridge/intel/gm45/gm45.h
@@ -420,7 +420,7 @@ void igd_compute_ggc(sysinfo_t *const sysinfo);
 int raminit_read_vco_index(void);
 u32 raminit_get_rank_addr(unsigned int channel, unsigned int rank);
 
-void raminit_rcomp_calibration(stepping_t stepping);
+void raminit_rcomp_calibration(int ddr_type, stepping_t stepping);
 void raminit_reset_readwrite_pointers(void);
 void raminit_receive_enable_calibration(int ddr_type, const timings_t *, const dimminfo_t *);
 void raminit_write_training(const mem_clock_t, const dimminfo_t *, int s3resume);
diff --git a/src/northbridge/intel/gm45/raminit.c b/src/northbridge/intel/gm45/raminit.c
index b7e013959a..df8f46fbbc 100644
--- a/src/northbridge/intel/gm45/raminit.c
+++ b/src/northbridge/intel/gm45/raminit.c
@@ -1047,7 +1047,7 @@ static void rcomp_initialization(const int spd_type, const stepping_t stepping,
 	}
 
 	/* Perform RCOMP calibration for DDR3. */
-	raminit_rcomp_calibration(stepping);
+	raminit_rcomp_calibration(spd_type, stepping);
 
 	/* Run initial RCOMP. */
 	mchbar_setbits32(0x418, 1 << 17);
@@ -1117,7 +1117,7 @@ static void dram_program_timings(const int spd_type, const timings_t *const timi
 				reg = (reg & ~(0xf << 10)) | (2 << 10);
 			else
 				reg = (reg & ~(0xf << 10)) | (3 << 10);
-			reg = (reg & ~(0x7 <<  5)) | (3 << 5);
+			reg = (reg & ~(0x7 <<  5)) | (2 << 5);
 		} else if (timings->mem_clock != MEM_CLOCK_1067MT) {
 			reg = (reg & ~(0x7 << 15)) | ((9 - timings->CAS) << 15);
 			reg = (reg & ~(0xf << 10)) | ((timings->CAS - 3) << 10);
@@ -1286,11 +1286,11 @@ static void ddr2_odt_setup(const timings_t *const timings, const int sff)
 		reg = (reg & ~(0xf << (44 - 32))) | (8 << (44 - 32));
 		reg = (reg & ~(0xf << (40 - 32))) | (7 << (40 - 32));
 		if (timings->mem_clock == MEM_CLOCK_667MT) {
-			reg = (reg & ~(0xf << (36 - 32))) | (4 << (36 - 32));
-			reg = (reg & ~(0xf << (32 - 32))) | (4 << (32 - 32));
+			reg = (reg & ~(0xf << (36 - 32))) | (8 << (36 - 32));
+			reg = (reg & ~(0xf << (32 - 32))) | (8 << (32 - 32));
 		} else {
-			reg = (reg & ~(0xf << (36 - 32))) | (5 << (36 - 32));
-			reg = (reg & ~(0xf << (32 - 32))) | (5 << (32 - 32));
+			reg = (reg & ~(0xf << (36 - 32))) | (9 << (36 - 32));
+			reg = (reg & ~(0xf << (32 - 32))) | (9 << (32 - 32));
 		}
 		mchbar_write32(CxODT_HIGH(ch), reg);
 
@@ -2209,6 +2209,84 @@ void raminit(sysinfo_t *const sysinfo, const int s3resume)
 		raminit_write_training(timings->mem_clock, dimms, s3resume);
 	}
 
+	/*
+	 * Program hardcoded DDR2-800 RCOMP SRAM codes. This must be done
+	 * after receiver enable calibration, otherwise raminit sometimes
+	 * completes with non-working memory.
+	 */
+	mchbar_write32(0x0530, 0x06060005);
+	mchbar_write32(0x0680, 0x06060606);
+	mchbar_write32(0x0684, 0x08070606);
+	mchbar_write32(0x0688, 0x0e0e0c0a);
+	mchbar_write32(0x068c, 0x0e0e0e0e);
+	mchbar_write32(0x0698, 0x06060606);
+	mchbar_write32(0x069c, 0x08070606);
+	mchbar_write32(0x06a0, 0x0c0c0b0a);
+	mchbar_write32(0x06a4, 0x0c0c0c0c);
+
+	mchbar_write32(0x06c0, 0x02020202);
+	mchbar_write32(0x06c4, 0x03020202);
+	mchbar_write32(0x06c8, 0x04040403);
+	mchbar_write32(0x06cc, 0x04040404);
+	mchbar_write32(0x06d8, 0x02020202);
+	mchbar_write32(0x06dc, 0x03020202);
+	mchbar_write32(0x06e0, 0x04040403);
+	mchbar_write32(0x06e4, 0x04040404);
+
+	mchbar_write32(0x0700, 0x02020202);
+	mchbar_write32(0x0704, 0x03020202);
+	mchbar_write32(0x0708, 0x04040403);
+	mchbar_write32(0x070c, 0x04040404);
+	mchbar_write32(0x0718, 0x02020202);
+	mchbar_write32(0x071c, 0x03020202);
+	mchbar_write32(0x0720, 0x04040403);
+	mchbar_write32(0x0724, 0x04040404);
+
+	mchbar_write32(0x0740, 0x02020202);
+	mchbar_write32(0x0744, 0x03020202);
+	mchbar_write32(0x0748, 0x04040403);
+	mchbar_write32(0x074c, 0x04040404);
+	mchbar_write32(0x0758, 0x02020202);
+	mchbar_write32(0x075c, 0x03020202);
+	mchbar_write32(0x0760, 0x04040403);
+	mchbar_write32(0x0764, 0x04040404);
+
+	mchbar_write32(0x0780, 0x06060606);
+	mchbar_write32(0x0784, 0x09070606);
+	mchbar_write32(0x0788, 0x0e0e0c0b);
+	mchbar_write32(0x078c, 0x0e0e0e0e);
+	mchbar_write32(0x0798, 0x06060606);
+	mchbar_write32(0x079c, 0x09070606);
+	mchbar_write32(0x07a0, 0x0d0d0c0b);
+	mchbar_write32(0x07a4, 0x0d0d0d0d);
+
+	mchbar_write32(0x07c0, 0x06060606);
+	mchbar_write32(0x07c4, 0x09070606);
+	mchbar_write32(0x07c8, 0x0e0e0c0b);
+	mchbar_write32(0x07cc, 0x0e0e0e0e);
+	mchbar_write32(0x07d8, 0x06060606);
+	mchbar_write32(0x07dc, 0x09070606);
+	mchbar_write32(0x07e0, 0x0d0d0c0b);
+	mchbar_write32(0x07e4, 0x0d0d0d0d);
+
+	mchbar_write32(0x0840, 0x06060606);
+	mchbar_write32(0x0844, 0x08070606);
+	mchbar_write32(0x0848, 0x0e0e0c0a);
+	mchbar_write32(0x084c, 0x0e0e0e0e);
+	mchbar_write32(0x0858, 0x06060606);
+	mchbar_write32(0x085c, 0x08070606);
+	mchbar_write32(0x0860, 0x0c0c0b0a);
+	mchbar_write32(0x0864, 0x0c0c0c0c);
+
+	mchbar_write32(0x0880, 0x02020202);
+	mchbar_write32(0x0884, 0x03020202);
+	mchbar_write32(0x0888, 0x04040403);
+	mchbar_write32(0x088c, 0x04040404);
+	mchbar_write32(0x0898, 0x02020202);
+	mchbar_write32(0x089c, 0x03020202);
+	mchbar_write32(0x08a0, 0x04040403);
+	mchbar_write32(0x08a4, 0x04040404);
+
 	igd_compute_ggc(sysinfo);
 
 	/* Program final memory map (with real values). */
diff --git a/src/northbridge/intel/gm45/raminit_rcomp_calibration.c b/src/northbridge/intel/gm45/raminit_rcomp_calibration.c
index aef863f05a..b74765fd9c 100644
--- a/src/northbridge/intel/gm45/raminit_rcomp_calibration.c
+++ b/src/northbridge/intel/gm45/raminit_rcomp_calibration.c
@@ -161,11 +161,13 @@ static void lookup_and_write(const int a1step,
 		mchbar += 4;
 	}
 }
-void raminit_rcomp_calibration(const stepping_t stepping) {
+void raminit_rcomp_calibration(int ddr_type, const stepping_t stepping) {
 	const int a1step = stepping >= STEPPING_CONVERSION_A1;
 
 	int i;
 
+	char magic_comp[2] = {0};
+
 	enum {
 		PULL_UP = 0,
 		PULL_DOWN = 1,
@@ -196,6 +198,10 @@ void raminit_rcomp_calibration(const stepping_t stepping) {
 		reg = mchbar_read32(0x518);
 		lut_idx[channel][group][PULL_UP] = (reg >> 24) & 0x7f;
 		lut_idx[channel][group][PULL_DOWN] = (reg >> 16) & 0x7f;
+		if (i == 1) {
+			magic_comp[0] = (reg >> 8) & 0x3f;
+			magic_comp[1] = (reg >> 0) & 0x3f;
+		}
 	}
 	/* Cleanup? */
 	mchbar_setbits32(0x400, 1 << 3);
@@ -216,13 +222,19 @@ void raminit_rcomp_calibration(const stepping_t stepping) {
 	for (channel = 0; channel < 2; ++channel) {
 		for (group = 0; group < 6; ++group) {
 			for (pu_pd = PULL_DOWN; pu_pd >= PULL_UP; --pu_pd) {
-				lookup_and_write(
-					a1step,
-					lut_idx[channel][group][pu_pd] - 7,
-					ddr3_lookup_schedule[group][pu_pd],
-					mchbar);
+				if (ddr_type == DDR3) {
+					lookup_and_write(
+						a1step,
+						lut_idx[channel][group][pu_pd] - 7,
+						ddr3_lookup_schedule[group][pu_pd],
+						mchbar);
+				}
 				mchbar += 0x0018;
 			}
+			if (ddr_type == DDR2) {
+				mchbar_clrsetbits32(mchbar + 0, 0x7f << 24, lut_idx[channel][group][PULL_DOWN] << 24);
+				mchbar_clrsetbits32(mchbar + 4, 0x7f <<  0, lut_idx[channel][group][PULL_UP]   <<  0);
+			}
 			mchbar += 0x0010;
 			/* Channel B knows only the first two groups. */
 			if ((1 == channel) && (1 == group))
@@ -230,4 +242,7 @@ void raminit_rcomp_calibration(const stepping_t stepping) {
 		}
 		mchbar += 0x0040;
 	}
+
+	mchbar_clrsetbits32(0x4d0, 0x3f << 26, magic_comp[0] << 26);
+	mchbar_clrsetbits32(0x4d0, 0x3f << 20, magic_comp[1] << 20);
 }
-- 
2.47.3

