From 0889cc6b6f62cba616feff5ae8558be31f298069 Mon Sep 17 00:00:00 2001
From: Nicholas Chin <nic.c3.14@gmail.com>
Date: Fri, 8 Mar 2024 09:33:03 -0700
Subject: [PATCH 16/51] mb/dell: Add Latitude E6330 (Ivy Bridge)

Mainboard is QAL70/LA-7741P. I do not physically have this system;
someone with physical access to one sent me the output of autoport which
I then modified to produce this port. I was also sent the VBT binary,
which was obtained from `/sys/kernel/debug/dri/0/i915_vbt` while running
version A21 of the vendor firmware. This port has not been tested.

The EC is the SMSC MEC5055, which seems to be compatible with the
existing MEC5035 code. As with the other Dell systems with this EC, this
board is assumed to be internally flashable using an EC command that
tells it to pull the FDO pin low on the next boot, which also tells the
vendor firmware to disable all write protections to the flash [1].

[1] https://gitlab.com/nic3-14159/dell-flash-unlock

Change-Id: I827826e9ff8a9a534c50250458b399104478e06c
Signed-off-by: Nicholas Chin <nic.c3.14@gmail.com>
---
 src/mainboard/dell/snb_ivb_latitude/Kconfig   |  11 +-
 .../dell/snb_ivb_latitude/Kconfig.name        |   3 +
 .../snb_ivb_latitude/variants/e6330/data.vbt  | Bin 0 -> 6144 bytes
 .../variants/e6330/early_init.c               |  14 ++
 .../snb_ivb_latitude/variants/e6330/gpio.c    | 192 ++++++++++++++++++
 .../variants/e6330/hda_verb.c                 |  32 +++
 .../variants/e6330/overridetree.cb            |  37 ++++
 7 files changed, 288 insertions(+), 1 deletion(-)
 create mode 100644 src/mainboard/dell/snb_ivb_latitude/variants/e6330/data.vbt
 create mode 100644 src/mainboard/dell/snb_ivb_latitude/variants/e6330/early_init.c
 create mode 100644 src/mainboard/dell/snb_ivb_latitude/variants/e6330/gpio.c
 create mode 100644 src/mainboard/dell/snb_ivb_latitude/variants/e6330/hda_verb.c
 create mode 100644 src/mainboard/dell/snb_ivb_latitude/variants/e6330/overridetree.cb

diff --git a/src/mainboard/dell/snb_ivb_latitude/Kconfig b/src/mainboard/dell/snb_ivb_latitude/Kconfig
index baa83baa41..49bf225fe2 100644
--- a/src/mainboard/dell/snb_ivb_latitude/Kconfig
+++ b/src/mainboard/dell/snb_ivb_latitude/Kconfig
@@ -56,6 +56,12 @@ config BOARD_DELL_LATITUDE_E5530
 	select BOARD_ROMSIZE_KB_12288
 	select SOUTHBRIDGE_INTEL_C216
 
+config BOARD_DELL_LATITUDE_E6330
+	select BOARD_DELL_SNB_IVB_LATITUDE_COMMON
+	select BOARD_ROMSIZE_KB_12288
+	select MAINBOARD_USES_IFD_GBE_REGION
+	select SOUTHBRIDGE_INTEL_C216
+
 config BOARD_DELL_LATITUDE_E6430
 	select BOARD_DELL_SNB_IVB_LATITUDE_COMMON
 	select BOARD_ROMSIZE_KB_12288
@@ -84,6 +90,7 @@ config MAINBOARD_PART_NUMBER
 	default "Latitude E6420" if BOARD_DELL_LATITUDE_E6420
 	default "Latitude E6520" if BOARD_DELL_LATITUDE_E6520
 	default "Latitude E5530" if BOARD_DELL_LATITUDE_E5530
+	default "Latitude E6330" if BOARD_DELL_LATITUDE_E6330
 	default "Latitude E6430" if BOARD_DELL_LATITUDE_E6430
 	default "Latitude E6530" if BOARD_DELL_LATITUDE_E6530
 
@@ -101,13 +108,15 @@ config VARIANT_DIR
 	default "e6420" if BOARD_DELL_LATITUDE_E6420
 	default "e6520" if BOARD_DELL_LATITUDE_E6520
 	default "e5530" if BOARD_DELL_LATITUDE_E5530
+	default "e6330" if BOARD_DELL_LATITUDE_E6330
 	default "e6430" if BOARD_DELL_LATITUDE_E6430
 	default "e6530" if BOARD_DELL_LATITUDE_E6530
 
 config VGA_BIOS_ID
 	default "8086,0116" if BOARD_DELL_LATITUDE_E6520 \
 		|| BOARD_DELL_LATITUDE_E5420
-	default "8086,0166" if BOARD_DELL_LATITUDE_E5530
+	default "8086,0166" if BOARD_DELL_LATITUDE_E5530 \
+		|| BOARD_DELL_LATITUDE_E6330
 	default "8086,0126" if BOARD_DELL_LATITUDE_E6420 \
 		|| BOARD_DELL_LATITUDE_E5520 \
 		|| BOARD_DELL_LATITUDE_E6220 \
diff --git a/src/mainboard/dell/snb_ivb_latitude/Kconfig.name b/src/mainboard/dell/snb_ivb_latitude/Kconfig.name
index 349ee7f79e..d6fc8eb224 100644
--- a/src/mainboard/dell/snb_ivb_latitude/Kconfig.name
+++ b/src/mainboard/dell/snb_ivb_latitude/Kconfig.name
@@ -21,6 +21,9 @@ config BOARD_DELL_LATITUDE_E6520
 config BOARD_DELL_LATITUDE_E5530
 	bool "Latitude E5530"
 
+config BOARD_DELL_LATITUDE_E6330
+	bool "Latitude E6330"
+
 config BOARD_DELL_LATITUDE_E6430
 	bool "Latitude E6430"
 
diff --git a/src/mainboard/dell/snb_ivb_latitude/variants/e6330/data.vbt b/src/mainboard/dell/snb_ivb_latitude/variants/e6330/data.vbt
new file mode 100644
index 0000000000000000000000000000000000000000..18856746656058651c571ecbb3708e0543b19d62
GIT binary patch
literal 6144
zcmeHKU2GiH75-*tc6WAmW_LYygMSkDB*E^Q*zv5f7dLg)@$NQV2a{}!yImnfyvQ4D
z;n-$v0!RpNi<_o@ktI-@2a590stC0zRi%iRR%stvi&hAs3R<K}X~hFddB_6@s8W`5
zXJ!q~E{TOme<a`8@BW;7?l<?GIp@yo&H2<M-FZ0GKbBAR-Ekx}HvVOrhK1*2?{QsU
zQe#K%JeC=q96gpAKa#$keu^D99ee*0FfB=@F_0J<9-Ch-&BZ5r1T6`{$;1%Fm+qfk
zTr5pfAz@KB*NGlFzEGx2aqh%IxkQOuX*`{wy~+KQo+-}XSE7aaxko77OBtFgoh;4K
z(#-7f<x+WxmKSK)vQFgtt^L+?s+Z<V57E7|^TqOPX{mn0n<VLl#Yf7s_suL*Jl#VB
zmSyz~ScwEVTc-3vd2v6D&dt$;&{?91(o(5>vNXNl&<qW@AghW5NPYw#ha~-b0Dc7_
z6}t(eHgpwn6<HNi1Vcp^p-07-iXve~MTs!0A_ku!`4nKciajxJYXsOYuuT4N%smA!
zPazgl&bNRSrvAz|_6r3+B;r1=!7D;RUUw8Ke+vNt7E3`(BA-woPvJFBK^3Gzfh4Nk
zOX!J0PJNB)Mk&Z_i?S2ez+iItz=)m79LydX&rM9`3wPaJ`T92=Uv0;g-!<4*M6z%+
z*omwb#VI+CU&%iFS{_DGS;sE}7G4juqRMCww!+k6=+abJj4v>Dsr*z_6HAP5GJeST
znX2JD;{xLa#;c6KGychVn-L6YXkv6Qx)}Y8&ok1DI~ZSM6dCt39%QUAzRh@o@gqjy
zL0qZ&DhN8ZR3xu$a$Cd{oasU3DNp{CCl6f~PYlq!Hte;Ia0^wn8Vut7>Wl1)s`^E-
z1DhGx<x<9D%6jd%)5>zr8&7h}dMJ3~YBe;)!vVf-T&?{PoMvvRR{!67;Xhz^g^loX
zja+*c-KJJoxbsm3pTE4THs`cgD{Pt+ga3en-i$P#9Wsra(oqRMr;H$4{gxr)9eF(x
zg0v@a7aj}rA^Kf#sNb*>at^>P)5li%ycOq*4e;3~RUj$i1e8=rHi&<Y^Hc>Y_gP4=
zxz9^%q0dLXqC&Bq<&sDScZwvatjRxB=rcJJiYb?w#4Iy2KTk1F6T>T}E@(DNGa>5R
z7&Yv)JdHrRI};pfsKLVj=FE=U*=*T4#ncVktknoGelT||SDY`+9WI_IZE<i@7SnC8
zN6~Gyo=&><wpzE~>`_>@wb<-RI-lu(_~Oy_Zo6={Cdq!uw(fmyz_u^cB&~5IS7g`U
zdUC}N$J5-C)|`CfUO+?xptr@*hJW$ZhBZk%JaMh_<8!ZGj)z*WU9fcg2`>dT##_?q
z=Ksx}uxo3jTHTq%E1}97UECE@r}nt3I=3R(HOL7jNg>teSM-g$aU#`3jk}#qh;D?6
zw=CYuA2#mS+vU%0P&u8RCn4)$8VH-2uy#01%VG0WSX&Fz`LMYj)?N<NyJ1t)wHBQY
z=;pYt<#l>gH_zzWS)G2Pn=k3wYdU|DnWmxbG$>`5lZJMWL92%O14BD!(C-cNFNXFH
zgVc!G9?@=&(4mNVcSJiLq3=b^rz6@k5qdFVUW{m$A{2|7d!kxz)VSrcQt@4sDoq^f
z98hXm=YS~qbf<kwigD|YevaR}^`7Jy^x~4_g75ka=c0r}VJF2aEv{=ilPf-mNQBNI
zEMK3YKB+`*xOu>iR|LbzHLa*mLXlH${^b4c9%>9%)HO-?LA1gT0mlz!M}8&;(;^x|
z*H2<VyY>2;juB|7F+k?y(_2~3@STqQ@f^sqD2c8g3x>ciM%siMq~;pKwfE57kw2K@
z!-ZN0QTVOP@aA5@fEGKjy2+D`t?2KzpPyRQ`JcmHJoc(<#h<UT;@W$t_d{|;S>vyF
zewtgef*II~y;k>*B!+(8*blXsY-~kcJa9zG2yfcMCt+|-0ex$pY`h1<*#rEv=~*<+
ztV``Um!q33-Aap9fUshX^N~GS2@X3^U9+MwgYQ74^?~6&yU^#oY#cvC9R_}P2d<wN
zJvOE)Xr7A2n#3x14}2_g(YN^0+oYDbb#|V{ze3pzGb9FiF#6Ra&L}bT(ZOvswS7RY
zxLjWFRwWXHR5&={t;%K+Vkd6NX2iF<SF)LXv@y472OmG!_W%Ni*ZDuev-S0%b!dfW
wz4{IL!+uT9t2XI4@_L@?Ri*bc_<n8A+wHaowmq=zfo%_LdtloGpN<DU00~N<ApigX

literal 0
HcmV?d00001

diff --git a/src/mainboard/dell/snb_ivb_latitude/variants/e6330/early_init.c b/src/mainboard/dell/snb_ivb_latitude/variants/e6330/early_init.c
new file mode 100644
index 0000000000..ff83db095b
--- /dev/null
+++ b/src/mainboard/dell/snb_ivb_latitude/variants/e6330/early_init.c
@@ -0,0 +1,14 @@
+/* SPDX-License-Identifier: GPL-2.0-only */
+
+#include <bootblock_common.h>
+#include <device/pci_ops.h>
+#include <ec/dell/mec5035/mec5035.h>
+#include <southbridge/intel/bd82x6x/pch.h>
+
+void bootblock_mainboard_early_init(void)
+{
+	pci_write_config16(PCH_LPC_DEV, LPC_EN, CNF1_LPC_EN | MC_LPC_EN
+			| KBC_LPC_EN | FDD_LPC_EN | LPT_LPC_EN
+			| COMB_LPC_EN | COMA_LPC_EN);
+	mec5035_early_init();
+}
diff --git a/src/mainboard/dell/snb_ivb_latitude/variants/e6330/gpio.c b/src/mainboard/dell/snb_ivb_latitude/variants/e6330/gpio.c
new file mode 100644
index 0000000000..777570765a
--- /dev/null
+++ b/src/mainboard/dell/snb_ivb_latitude/variants/e6330/gpio.c
@@ -0,0 +1,192 @@
+/* SPDX-License-Identifier: GPL-2.0-only */
+
+#include <southbridge/intel/common/gpio.h>
+
+static const struct pch_gpio_set1 pch_gpio_set1_mode = {
+	.gpio0 = GPIO_MODE_GPIO,
+	.gpio1 = GPIO_MODE_GPIO,
+	.gpio2 = GPIO_MODE_GPIO,
+	.gpio3 = GPIO_MODE_GPIO,
+	.gpio4 = GPIO_MODE_GPIO,
+	.gpio5 = GPIO_MODE_NATIVE,
+	.gpio6 = GPIO_MODE_GPIO,
+	.gpio7 = GPIO_MODE_GPIO,
+	.gpio8 = GPIO_MODE_GPIO,
+	.gpio9 = GPIO_MODE_NATIVE,
+	.gpio10 = GPIO_MODE_NATIVE,
+	.gpio11 = GPIO_MODE_NATIVE,
+	.gpio12 = GPIO_MODE_NATIVE,
+	.gpio13 = GPIO_MODE_GPIO,
+	.gpio14 = GPIO_MODE_GPIO,
+	.gpio15 = GPIO_MODE_GPIO,
+	.gpio16 = GPIO_MODE_GPIO,
+	.gpio17 = GPIO_MODE_GPIO,
+	.gpio18 = GPIO_MODE_NATIVE,
+	.gpio19 = GPIO_MODE_GPIO,
+	.gpio20 = GPIO_MODE_NATIVE,
+	.gpio21 = GPIO_MODE_GPIO,
+	.gpio22 = GPIO_MODE_GPIO,
+	.gpio23 = GPIO_MODE_NATIVE,
+	.gpio24 = GPIO_MODE_GPIO,
+	.gpio25 = GPIO_MODE_NATIVE,
+	.gpio26 = GPIO_MODE_NATIVE,
+	.gpio27 = GPIO_MODE_GPIO,
+	.gpio28 = GPIO_MODE_GPIO,
+	.gpio29 = GPIO_MODE_GPIO,
+	.gpio30 = GPIO_MODE_NATIVE,
+	.gpio31 = GPIO_MODE_NATIVE,
+};
+
+static const struct pch_gpio_set1 pch_gpio_set1_direction = {
+	.gpio0 = GPIO_DIR_INPUT,
+	.gpio1 = GPIO_DIR_INPUT,
+	.gpio2 = GPIO_DIR_INPUT,
+	.gpio3 = GPIO_DIR_INPUT,
+	.gpio4 = GPIO_DIR_INPUT,
+	.gpio6 = GPIO_DIR_INPUT,
+	.gpio7 = GPIO_DIR_INPUT,
+	.gpio8 = GPIO_DIR_INPUT,
+	.gpio13 = GPIO_DIR_INPUT,
+	.gpio14 = GPIO_DIR_INPUT,
+	.gpio15 = GPIO_DIR_INPUT,
+	.gpio16 = GPIO_DIR_INPUT,
+	.gpio17 = GPIO_DIR_INPUT,
+	.gpio19 = GPIO_DIR_INPUT,
+	.gpio21 = GPIO_DIR_INPUT,
+	.gpio22 = GPIO_DIR_INPUT,
+	.gpio24 = GPIO_DIR_INPUT,
+	.gpio27 = GPIO_DIR_INPUT,
+	.gpio28 = GPIO_DIR_OUTPUT,
+	.gpio29 = GPIO_DIR_INPUT,
+};
+
+static const struct pch_gpio_set1 pch_gpio_set1_level = {
+	.gpio28 = GPIO_LEVEL_LOW,
+};
+
+static const struct pch_gpio_set1 pch_gpio_set1_reset = {
+	.gpio30 = GPIO_RESET_RSMRST,
+};
+
+static const struct pch_gpio_set1 pch_gpio_set1_invert = {
+	.gpio0 = GPIO_INVERT,
+	.gpio8 = GPIO_INVERT,
+	.gpio13 = GPIO_INVERT,
+	.gpio14 = GPIO_INVERT,
+};
+
+static const struct pch_gpio_set1 pch_gpio_set1_blink = {
+};
+
+static const struct pch_gpio_set2 pch_gpio_set2_mode = {
+	.gpio32 = GPIO_MODE_NATIVE,
+	.gpio33 = GPIO_MODE_GPIO,
+	.gpio34 = GPIO_MODE_GPIO,
+	.gpio35 = GPIO_MODE_GPIO,
+	.gpio36 = GPIO_MODE_GPIO,
+	.gpio37 = GPIO_MODE_GPIO,
+	.gpio38 = GPIO_MODE_GPIO,
+	.gpio39 = GPIO_MODE_GPIO,
+	.gpio40 = GPIO_MODE_NATIVE,
+	.gpio41 = GPIO_MODE_NATIVE,
+	.gpio42 = GPIO_MODE_NATIVE,
+	.gpio43 = GPIO_MODE_NATIVE,
+	.gpio44 = GPIO_MODE_NATIVE,
+	.gpio45 = GPIO_MODE_GPIO,
+	.gpio46 = GPIO_MODE_NATIVE,
+	.gpio47 = GPIO_MODE_NATIVE,
+	.gpio48 = GPIO_MODE_GPIO,
+	.gpio49 = GPIO_MODE_GPIO,
+	.gpio50 = GPIO_MODE_NATIVE,
+	.gpio51 = GPIO_MODE_GPIO,
+	.gpio52 = GPIO_MODE_GPIO,
+	.gpio53 = GPIO_MODE_NATIVE,
+	.gpio54 = GPIO_MODE_GPIO,
+	.gpio55 = GPIO_MODE_NATIVE,
+	.gpio56 = GPIO_MODE_NATIVE,
+	.gpio57 = GPIO_MODE_GPIO,
+	.gpio58 = GPIO_MODE_NATIVE,
+	.gpio59 = GPIO_MODE_NATIVE,
+	.gpio60 = GPIO_MODE_GPIO,
+	.gpio61 = GPIO_MODE_NATIVE,
+	.gpio62 = GPIO_MODE_NATIVE,
+	.gpio63 = GPIO_MODE_NATIVE,
+};
+
+static const struct pch_gpio_set2 pch_gpio_set2_direction = {
+	.gpio33 = GPIO_DIR_INPUT,
+	.gpio34 = GPIO_DIR_OUTPUT,
+	.gpio35 = GPIO_DIR_INPUT,
+	.gpio36 = GPIO_DIR_INPUT,
+	.gpio37 = GPIO_DIR_INPUT,
+	.gpio38 = GPIO_DIR_INPUT,
+	.gpio39 = GPIO_DIR_INPUT,
+	.gpio45 = GPIO_DIR_OUTPUT,
+	.gpio48 = GPIO_DIR_INPUT,
+	.gpio49 = GPIO_DIR_INPUT,
+	.gpio51 = GPIO_DIR_INPUT,
+	.gpio52 = GPIO_DIR_INPUT,
+	.gpio54 = GPIO_DIR_INPUT,
+	.gpio57 = GPIO_DIR_INPUT,
+	.gpio60 = GPIO_DIR_OUTPUT,
+};
+
+static const struct pch_gpio_set2 pch_gpio_set2_level = {
+	.gpio34 = GPIO_LEVEL_HIGH,
+	.gpio45 = GPIO_LEVEL_LOW,
+	.gpio60 = GPIO_LEVEL_HIGH,
+};
+
+static const struct pch_gpio_set2 pch_gpio_set2_reset = {
+};
+
+static const struct pch_gpio_set3 pch_gpio_set3_mode = {
+	.gpio64 = GPIO_MODE_NATIVE,
+	.gpio65 = GPIO_MODE_NATIVE,
+	.gpio66 = GPIO_MODE_NATIVE,
+	.gpio67 = GPIO_MODE_NATIVE,
+	.gpio68 = GPIO_MODE_GPIO,
+	.gpio69 = GPIO_MODE_GPIO,
+	.gpio70 = GPIO_MODE_GPIO,
+	.gpio71 = GPIO_MODE_GPIO,
+	.gpio72 = GPIO_MODE_NATIVE,
+	.gpio73 = GPIO_MODE_NATIVE,
+	.gpio74 = GPIO_MODE_NATIVE,
+	.gpio75 = GPIO_MODE_NATIVE,
+};
+
+static const struct pch_gpio_set3 pch_gpio_set3_direction = {
+	.gpio68 = GPIO_DIR_INPUT,
+	.gpio69 = GPIO_DIR_INPUT,
+	.gpio70 = GPIO_DIR_INPUT,
+	.gpio71 = GPIO_DIR_INPUT,
+};
+
+static const struct pch_gpio_set3 pch_gpio_set3_level = {
+};
+
+static const struct pch_gpio_set3 pch_gpio_set3_reset = {
+};
+
+const struct pch_gpio_map mainboard_gpio_map = {
+	.set1 = {
+		.mode		= &pch_gpio_set1_mode,
+		.direction	= &pch_gpio_set1_direction,
+		.level		= &pch_gpio_set1_level,
+		.blink		= &pch_gpio_set1_blink,
+		.invert		= &pch_gpio_set1_invert,
+		.reset		= &pch_gpio_set1_reset,
+	},
+	.set2 = {
+		.mode		= &pch_gpio_set2_mode,
+		.direction	= &pch_gpio_set2_direction,
+		.level		= &pch_gpio_set2_level,
+		.reset		= &pch_gpio_set2_reset,
+	},
+	.set3 = {
+		.mode		= &pch_gpio_set3_mode,
+		.direction	= &pch_gpio_set3_direction,
+		.level		= &pch_gpio_set3_level,
+		.reset		= &pch_gpio_set3_reset,
+	},
+};
diff --git a/src/mainboard/dell/snb_ivb_latitude/variants/e6330/hda_verb.c b/src/mainboard/dell/snb_ivb_latitude/variants/e6330/hda_verb.c
new file mode 100644
index 0000000000..804733b172
--- /dev/null
+++ b/src/mainboard/dell/snb_ivb_latitude/variants/e6330/hda_verb.c
@@ -0,0 +1,32 @@
+/* SPDX-License-Identifier: GPL-2.0-only */
+
+#include <device/azalia_device.h>
+
+const u32 cim_verb_data[] = {
+	0x111d76df,	/* Codec Vendor / Device ID: IDT */
+	0x10280533,	/* Subsystem ID */
+	11,		/* Number of 4 dword sets */
+	AZALIA_SUBVENDOR(0, 0x10280533),
+	AZALIA_PIN_CFG(0, 0x0a, 0x03a11020),
+	AZALIA_PIN_CFG(0, 0x0b, 0x0321101f),
+	AZALIA_PIN_CFG(0, 0x0c, 0x400000f0),
+	AZALIA_PIN_CFG(0, 0x0d, 0x90170110),
+	AZALIA_PIN_CFG(0, 0x0e, 0x23011050),
+	AZALIA_PIN_CFG(0, 0x0f, 0x23a1102e),
+	AZALIA_PIN_CFG(0, 0x10, 0x400000f3),
+	AZALIA_PIN_CFG(0, 0x11, 0xd5a30130),
+	AZALIA_PIN_CFG(0, 0x1f, 0x400000f0),
+	AZALIA_PIN_CFG(0, 0x20, 0x400000f0),
+
+	0x80862806,	/* Codec Vendor / Device ID: Intel */
+	0x80860101,	/* Subsystem ID */
+	4,		/* Number of 4 dword sets */
+	AZALIA_SUBVENDOR(3, 0x80860101),
+	AZALIA_PIN_CFG(3, 0x05, 0x18560010),
+	AZALIA_PIN_CFG(3, 0x06, 0x18560020),
+	AZALIA_PIN_CFG(3, 0x07, 0x18560030),
+};
+
+const u32 pc_beep_verbs[0] = {};
+
+AZALIA_ARRAY_SIZES;
diff --git a/src/mainboard/dell/snb_ivb_latitude/variants/e6330/overridetree.cb b/src/mainboard/dell/snb_ivb_latitude/variants/e6330/overridetree.cb
new file mode 100644
index 0000000000..4125159367
--- /dev/null
+++ b/src/mainboard/dell/snb_ivb_latitude/variants/e6330/overridetree.cb
@@ -0,0 +1,37 @@
+## SPDX-License-Identifier: GPL-2.0-or-later
+
+chip northbridge/intel/sandybridge
+	device domain 0 on
+		subsystemid 0x1028 0x0533 inherit
+
+		device ref igd on
+			register "gpu_cpu_backlight" = "0x00001312"
+			register "gpu_pch_backlight" = "0x13121312"
+		end
+
+		chip southbridge/intel/bd82x6x
+			register "usb_port_config" = "{
+				{ 1, 2, 0 },
+				{ 1, 0, 0 },
+				{ 1, 0, 1 },
+				{ 1, 1, 1 },
+				{ 1, 1, 2 },
+				{ 1, 1, 2 },
+				{ 1, 2, 3 },
+				{ 1, 2, 3 },
+				{ 1, 2, 4 },
+				{ 1, 1, 4 },
+				{ 1, 1, 5 },
+				{ 1, 1, 5 },
+				{ 1, 2, 6 },
+				{ 1, 0, 6 },
+			}"
+
+			device ref xhci on
+				register "superspeed_capable_ports" = "0x0000000f"
+				register "xhci_overcurrent_mapping" = "0x00000c03"
+				register "xhci_switchable_ports" = "0x0000000f"
+			end
+		end
+	end
+end
-- 
2.39.5

