From 926b1af1033c26ad231587fd3a4506efb4b0d8a3 Mon Sep 17 00:00:00 2001
From: Angel Pons <th3fanbus@gmail.com>
Date: Sun, 8 May 2022 01:11:03 +0200
Subject: [PATCH 39/51] haswell NRI: Add library to change margins

Implement a library to change Rx/Tx margins. It will be expanded later.

Change-Id: I0b55aba428d8b4d4e16d2fbdec57235ce3ce8adf
Signed-off-by: Angel Pons <th3fanbus@gmail.com>
---
 .../intel/haswell/native_raminit/Makefile.mk  |   1 +
 .../haswell/native_raminit/change_margin.c    | 154 ++++++++++++++++++
 .../haswell/native_raminit/raminit_native.h   |  50 ++++++
 .../intel/haswell/registers/mchbar.h          |   9 +
 4 files changed, 214 insertions(+)
 create mode 100644 src/northbridge/intel/haswell/native_raminit/change_margin.c

diff --git a/src/northbridge/intel/haswell/native_raminit/Makefile.mk b/src/northbridge/intel/haswell/native_raminit/Makefile.mk
index 2da950771d..ebe9e9b762 100644
--- a/src/northbridge/intel/haswell/native_raminit/Makefile.mk
+++ b/src/northbridge/intel/haswell/native_raminit/Makefile.mk
@@ -1,5 +1,6 @@
 ## SPDX-License-Identifier: GPL-2.0-or-later
 
+romstage-y += change_margin.c
 romstage-y += configure_mc.c
 romstage-y += ddr3.c
 romstage-y += jedec_reset.c
diff --git a/src/northbridge/intel/haswell/native_raminit/change_margin.c b/src/northbridge/intel/haswell/native_raminit/change_margin.c
new file mode 100644
index 0000000000..055c666eee
--- /dev/null
+++ b/src/northbridge/intel/haswell/native_raminit/change_margin.c
@@ -0,0 +1,154 @@
+/* SPDX-License-Identifier: GPL-2.0-or-later */
+
+#include <commonlib/bsd/clamp.h>
+#include <console/console.h>
+#include <delay.h>
+#include <northbridge/intel/haswell/haswell.h>
+#include <timer.h>
+
+#include "raminit_native.h"
+
+void update_rxt(
+	struct sysinfo *ctrl,
+	const uint8_t channel,
+	const uint8_t rank,
+	const uint8_t byte,
+	const enum rxt_subfield subfield,
+	const int32_t value)
+{
+	union ddr_data_rx_train_rank_reg rxt = {
+		.rcven =  ctrl->rcven[channel][rank][byte],
+		.dqs_p = ctrl->rxdqsp[channel][rank][byte],
+		.rx_eq =  ctrl->rx_eq[channel][rank][byte],
+		.dqs_n = ctrl->rxdqsn[channel][rank][byte],
+		.vref  = ctrl->rxvref[channel][rank][byte],
+	};
+	int32_t new_value;
+	switch (subfield) {
+	case RXT_RCVEN:
+		new_value = clamp_s32(0, value, 511);
+		rxt.rcven = new_value;
+		break;
+	case RXT_RXDQS_P:
+		new_value = clamp_s32(0, value, 63);
+		rxt.dqs_p = new_value;
+		break;
+	case RXT_RX_EQ:
+		new_value = clamp_s32(0, value, 31);
+		rxt.rx_eq = new_value;
+		break;
+	case RXT_RXDQS_N:
+		new_value = clamp_s32(0, value, 63);
+		rxt.dqs_n = new_value;
+		break;
+	case RXT_RX_VREF:
+		new_value = clamp_s32(-32, value, 31);
+		rxt.vref = new_value;
+		break;
+	case RXT_RXDQS_BOTH:
+		new_value = clamp_s32(0, value, 63);
+		rxt.dqs_p = new_value;
+		rxt.dqs_n = new_value;
+		break;
+	case RXT_RESTORE:
+		new_value = value;
+		break;
+	default:
+		die("%s: Unhandled subfield index %u\n", __func__, subfield);
+	}
+
+	if (new_value != value) {
+		printk(BIOS_ERR, "%s: Overflow for subfield %u: %d ---> %d\n",
+			__func__, subfield, value, new_value);
+	}
+	mchbar_write32(RX_TRAIN_ch_r_b(channel, rank, byte), rxt.raw);
+	download_regfile(ctrl, channel, false, rank, REG_FILE_USE_RANK, byte, true, false);
+}
+
+void update_txt(
+	struct sysinfo *ctrl,
+	const uint8_t channel,
+	const uint8_t rank,
+	const uint8_t byte,
+	const enum txt_subfield subfield,
+	const int32_t value)
+{
+	union ddr_data_tx_train_rank_reg txt = {
+		.dq_delay  = ctrl->tx_dq[channel][rank][byte],
+		.dqs_delay = ctrl->txdqs[channel][rank][byte],
+		.tx_eq     = ctrl->tx_eq[channel][rank][byte],
+	};
+	int32_t new_value;
+	switch (subfield) {
+	case TXT_TX_DQ:
+		new_value = clamp_s32(0, value, 511);
+		txt.dq_delay = new_value;
+		break;
+	case TXT_TXDQS:
+		new_value = clamp_s32(0, value, 511);
+		txt.dqs_delay = new_value;
+		break;
+	case TXT_TX_EQ:
+		new_value = clamp_s32(0, value, 63);
+		txt.tx_eq = new_value;
+		break;
+	case TXT_DQDQS_OFF:
+		new_value = value;
+		txt.dqs_delay += new_value;
+		txt.dq_delay  += new_value;
+		break;
+	case TXT_RESTORE:
+		new_value = value;
+		break;
+	default:
+		die("%s: Unhandled subfield index %u\n", __func__, subfield);
+	}
+	if (new_value != value) {
+		printk(BIOS_ERR, "%s: Overflow for subfield %u: %d ---> %d\n",
+			__func__, subfield, value, new_value);
+	}
+	mchbar_write32(TX_TRAIN_ch_r_b(channel, rank, byte), txt.raw);
+	download_regfile(ctrl, channel, false, rank, REG_FILE_USE_RANK, byte, false, true);
+}
+
+void download_regfile(
+	struct sysinfo *ctrl,
+	const uint8_t channel,
+	const bool multicast,
+	const uint8_t rank,
+	const enum regfile_mode regfile,
+	const uint8_t byte,
+	const bool read_rf_rd,
+	const bool read_rf_wr)
+{
+	union reut_seq_base_addr_reg reut_seq_base_addr;
+	switch (regfile) {
+	case REG_FILE_USE_START:
+		reut_seq_base_addr.raw = mchbar_read64(REUT_ch_SEQ_ADDR_START(channel));
+		break;
+	case REG_FILE_USE_CURRENT:
+		reut_seq_base_addr.raw = mchbar_read64(REUT_ch_SEQ_ADDR_CURRENT(channel));
+		break;
+	case REG_FILE_USE_RANK:
+		reut_seq_base_addr.raw = 0;
+		if (rank >= NUM_SLOTRANKS)
+			die("%s: bad rank %u\n", __func__, rank);
+		break;
+	default:
+		die("%s: Invalid regfile param %u\n", __func__, regfile);
+	}
+	uint8_t phys_rank = rank;
+	if (reut_seq_base_addr.raw != 0) {
+		/* Map REUT logical rank to physical rank */
+		const uint32_t log_to_phys = mchbar_read32(REUT_ch_RANK_LOG_TO_PHYS(channel));
+		phys_rank = log_to_phys >> (reut_seq_base_addr.rank_addr * 4) & 0x3;
+	}
+	uint32_t reg = multicast ? DDR_DATA_ch_CONTROL_0(channel) : DQ_CONTROL_0(channel, byte);
+	union ddr_data_control_0_reg ddr_data_control_0 = {
+		.raw = mchbar_read32(reg),
+	};
+	ddr_data_control_0.read_rf_rd   = read_rf_rd;
+	ddr_data_control_0.read_rf_wr   = read_rf_wr;
+	ddr_data_control_0.read_rf_rank = phys_rank;
+	mchbar_write32(reg, ddr_data_control_0.raw);
+}
diff --git a/src/northbridge/intel/haswell/native_raminit/raminit_native.h b/src/northbridge/intel/haswell/native_raminit/raminit_native.h
index f029e7f076..8707257b27 100644
--- a/src/northbridge/intel/haswell/native_raminit/raminit_native.h
+++ b/src/northbridge/intel/haswell/native_raminit/raminit_native.h
@@ -118,6 +118,30 @@ enum test_stop {
 	ALSOE  = 3,	/* Stop on all lanes error */
 };
 
+enum rxt_subfield {
+	RXT_RCVEN	= 0,
+	RXT_RXDQS_P	= 1,
+	RXT_RX_EQ	= 2,
+	RXT_RXDQS_N	= 3,
+	RXT_RX_VREF	= 4,
+	RXT_RXDQS_BOTH	= 5,
+	RXT_RESTORE	= 255,
+};
+
+enum txt_subfield {
+	TXT_TX_DQ	= 0,
+	TXT_TXDQS	= 1,
+	TXT_TX_EQ	= 2,
+	TXT_DQDQS_OFF	= 3,
+	TXT_RESTORE	= 255,
+};
+
+enum regfile_mode {
+	REG_FILE_USE_RANK,	/* Used when changing parameters for each rank */
+	REG_FILE_USE_START,	/* Used when changing parameters before the test */
+	REG_FILE_USE_CURRENT,	/* Used when changing parameters after the test */
+};
+
 struct wdb_pat {
 	uint32_t start_ptr;	/* Starting pointer in WDB */
 	uint32_t stop_ptr;	/* Stopping pointer in WDB */
@@ -451,6 +475,32 @@ uint8_t select_reut_ranks(struct sysinfo *ctrl, uint8_t channel, uint8_t rankmas
 void run_mpr_io_test(bool clear_errors);
 uint8_t run_io_test(struct sysinfo *ctrl, uint8_t chanmask, uint8_t dq_pat, bool clear_errors);
 
+void update_rxt(
+	struct sysinfo *ctrl,
+	uint8_t channel,
+	uint8_t rank,
+	uint8_t byte,
+	enum rxt_subfield subfield,
+	int32_t value);
+
+void update_txt(
+	struct sysinfo *ctrl,
+	uint8_t channel,
+	uint8_t rank,
+	uint8_t byte,
+	enum txt_subfield subfield,
+	int32_t value);
+
+void download_regfile(
+	struct sysinfo *ctrl,
+	uint8_t channel,
+	bool multicast,
+	uint8_t rank,
+	enum regfile_mode regfile,
+	uint8_t byte,
+	bool read_rf_rd,
+	bool read_rf_wr);
+
 uint8_t get_rx_bias(const struct sysinfo *ctrl);
 
 uint8_t get_tCWL(uint32_t mem_clock_mhz);
diff --git a/src/northbridge/intel/haswell/registers/mchbar.h b/src/northbridge/intel/haswell/registers/mchbar.h
index 817a9f8bf8..a81559bb1e 100644
--- a/src/northbridge/intel/haswell/registers/mchbar.h
+++ b/src/northbridge/intel/haswell/registers/mchbar.h
@@ -15,7 +15,11 @@
 /* Register definitions */
 
 /* DDR DATA per-channel per-bytelane */
+#define RX_TRAIN_ch_r_b(ch, rank, byte)		_DDRIO_C_R_B(0x0000, ch, rank, byte)
+#define TX_TRAIN_ch_r_b(ch, rank, byte)		_DDRIO_C_R_B(0x0020, ch, rank, byte)
+
 #define DQ_CONTROL_2(ch, byte)			_DDRIO_C_R_B(0x0064, ch, 0, byte)
+#define DQ_CONTROL_0(ch, byte)			_DDRIO_C_R_B(0x0074, ch, 0, byte)
 
 /* DDR CKE per-channel */
 #define DDR_CKE_ch_CMD_COMP_OFFSET(ch)		_DDRIO_C_R_B(0x1204, ch, 0, 0)
@@ -38,6 +42,9 @@
 #define DDR_SCRAMBLE_ch(ch)			(0x2000 + 4 * (ch))
 #define DDR_SCRAM_MISC_CONTROL			0x2008
 
+/* DDR DATA per-channel multicast */
+#define DDR_DATA_ch_CONTROL_0(ch)		_DDRIO_C_R_B(0x3074, ch, 0, 0)
+
 /* DDR CMDN/CMDS per-channel (writes go to both CMDN and CMDS fubs) */
 #define DDR_CMD_ch_COMP_OFFSET(ch)		_DDRIO_C_R_B(0x3204, ch, 0, 0)
 #define DDR_CMD_ch_PI_CODING(ch)		_DDRIO_C_R_B(0x3208, ch, 0, 0)
@@ -147,6 +154,8 @@
 
 #define REUT_ch_SEQ_ADDR_WRAP(ch)		(0x48e8 + 8 * (ch))
 
+#define REUT_ch_SEQ_ADDR_CURRENT(ch)		(0x48f8 + 8 * (ch))
+
 #define REUT_ch_SEQ_MISC_CTL(ch)		(0x4908 + 4 * (ch))
 
 #define REUT_ch_SEQ_ADDR_INC_CTL(ch)		(0x4910 + 8 * (ch))
-- 
2.39.5

