From d02163324baeb817ed55df41fac863cab4be038c Mon Sep 17 00:00:00 2001
From: Alper Nebi Yasak <alpernebiyasak@gmail.com>
Date: Wed, 10 Jul 2024 14:32:19 +0300
Subject: [PATCH] HACK: rk3399: gru: Remove assigned clock dt properties for
 EDP node

Having the PCLK_EDP clock in the assigned-clocks property of the `edp`
node means that U-Boot tries to set its rate automatically. This clock
isn't implemented for the RK3399 clock driver, so it fails and prevents
display from being initialized.

The display happens to work fine without it, remove the property until
the clock driver can handle the clock.

Signed-off-by: Alper Nebi Yasak <alpernebiyasak@gmail.com>
---
 arch/arm/dts/rk3399-gru-u-boot.dtsi | 3 +++
 1 file changed, 3 insertions(+)

diff --git a/arch/arm/dts/rk3399-gru-u-boot.dtsi b/arch/arm/dts/rk3399-gru-u-boot.dtsi
index 5517176aa4a0..9f40cf1e0208 100644
--- a/arch/arm/dts/rk3399-gru-u-boot.dtsi
+++ b/arch/arm/dts/rk3399-gru-u-boot.dtsi
@@ -27,6 +27,9 @@ &cros_ec {
 
 &edp {
 	rockchip,panel = <&edp_panel>;
+
+	/delete-property/ assigned-clocks;
+	/delete-property/ assigned-clock-rates;
 };
 
 &emmc_phy {
-- 
2.49.0

