From e564490781b0b829da43534c6c2a1b26aeb3282f Mon Sep 17 00:00:00 2001
From: Leah Rowe <leah@libreboot.org>
Date: Sat, 4 Oct 2025 22:20:11 +0100
Subject: [PATCH 39/40] alderlake: don't require full fsp repo for fd path

Signed-off-by: Leah Rowe <leah@libreboot.org>
---
 src/soc/intel/alderlake/Kconfig | 9 ++++++++-
 1 file changed, 8 insertions(+), 1 deletion(-)

diff --git a/src/soc/intel/alderlake/Kconfig b/src/soc/intel/alderlake/Kconfig
index 1f6a1dca7d..3979d9e162 100644
--- a/src/soc/intel/alderlake/Kconfig
+++ b/src/soc/intel/alderlake/Kconfig
@@ -415,7 +415,14 @@ config FSP_HEADER_PATH
 
 config FSP_FD_PATH
 	string
-	depends on FSP_USE_REPO
+#	dependency removed for lbmk purposes, so that the path is present
+#	in the config regardless of whether it's used. this is for ./mk -d
+#	on alderlake boards, which is used by lbmk to manually split fsp,
+#	even though the result is identical to what coreboot produces, because
+#	this enables lbmk to strip the fsp in release archives, and re-insert
+#	for compliance reasons (due to technicalities in intel's licensing),
+#	and to enable lbmk's advanced checksum verification of vendor files
+#	depends on FSP_USE_REPO
 	default "3rdparty/fsp/RaptorLakeFspBinPkg/IoT/RaptorLakeP/FSP.fd"   if FSP_TYPE_IOT && SOC_INTEL_ALDERLAKE_PCH_P && SOC_INTEL_RAPTORLAKE
 	default "3rdparty/fsp/RaptorLakeFspBinPkg/IoT/RaptorLakeS/FSP.fd"   if FSP_TYPE_IOT && SOC_INTEL_RAPTORLAKE_PCH_S
 	default "3rdparty/fsp/AlderLakeFspBinPkg/IoT/AlderLakeP/Fsp.fd"     if FSP_TYPE_IOT && SOC_INTEL_ALDERLAKE_PCH_P
-- 
2.47.3

